# Arduino Settings
CONFIG_FREERTOS_HZ=1000
CONFIG_AUTOSTART_ARDUINO=y

# Log Levels
# Boot Messages - Log level
CONFIG_BOOTLOADER_LOG_LEVEL_ERROR=y
# Arduino Log Level
CONFIG_ARDUHAL_LOG_DEFAULT_LEVEL_VERBOSE=y
# IDF Log Level
CONFIG_LOG_DEFAULT_LEVEL_WARN=y

#enable BT
CONFIG_BT_ENABLED=y
CONFIG_BT_NIMBLE_ENABLED=y

#disable BT connection reattempt
CONFIG_BT_NIMBLE_ENABLE_CONN_REATTEMPT=n

#enable lwip ipv6 autoconfig
CONFIG_LWIP_IPV6_AUTOCONFIG=y

# Use a custom partition table
CONFIG_PARTITION_TABLE_CUSTOM=y
CONFIG_PARTITION_TABLE_FILENAME="partitions.csv"
CONFIG_PARTITION_TABLE_OFFSET=0xC000

# Disable chip shell
CONFIG_ENABLE_CHIP_SHELL=n

#enable lwIP route hooks
CONFIG_LWIP_HOOK_IP6_ROUTE_DEFAULT=y
CONFIG_LWIP_HOOK_ND6_GET_GW_DEFAULT=y

# Button
CONFIG_BUTTON_PERIOD_TIME_MS=20
CONFIG_BUTTON_LONG_PRESS_TIME_MS=5000

# disable softap by default
CONFIG_ESP_WIFI_SOFTAP_SUPPORT=n

# Disable DS Peripheral
CONFIG_ESP_SECURE_CERT_DS_PERIPHERAL=n

# Use compact attribute storage mode
CONFIG_ESP_MATTER_NVS_USE_COMPACT_ATTR_STORAGE=y

# Enable HKDF in mbedtls
CONFIG_MBEDTLS_HKDF_C=y

# Increase LwIP IPv6 address number to 6 (MAX_FABRIC + 1)
# unique local addresses for fabrics(MAX_FABRIC), a link local address(1)
CONFIG_LWIP_IPV6_NUM_ADDRESSES=6


# ESP32-S3-DevKitC-1 Settings
# Buttons
CONFIG_BSP_BUTTONS_NUM=1
CONFIG_BSP_BUTTON_1_TYPE_GPIO=y
CONFIG_BSP_BUTTON_1_GPIO=0
CONFIG_BSP_BUTTON_1_LEVEL=0
# LEDs
CONFIG_BSP_LEDS_NUM=1
CONFIG_BSP_LED_TYPE_RGB=y
CONFIG_BSP_LED_RGB_GPIO=48
CONFIG_BSP_LED_RGB_BACKEND_RMT=y