CONFIG_IDF_TARGET="esp32s3"

# Arduino Settings
CONFIG_FREERTOS_HZ=1000
CONFIG_AUTOSTART_ARDUINO=y

# Log Levels
# Boot Messages - Log level 
CONFIG_BOOTLOADER_LOG_LEVEL_ERROR=y
# Arduino Log Level
CONFIG_ARDUHAL_LOG_DEFAULT_LEVEL_INFO=y
# IDF Log Level
CONFIG_LOG_DEFAULT_LEVEL_ERROR=y

# Default to 921600 baud when flashing and monitoring device
CONFIG_ESPTOOLPY_BAUD_921600B=y
CONFIG_ESPTOOLPY_BAUD=921600
CONFIG_ESPTOOLPY_COMPRESSED=y
CONFIG_ESPTOOLPY_MONITOR_BAUD_115200B=y
CONFIG_ESPTOOLPY_MONITOR_BAUD=115200
CONFIG_ESPTOOLPY_FLASHSIZE_4MB=y

#enable BT
CONFIG_BT_ENABLED=y
CONFIG_BT_NIMBLE_ENABLED=y

#disable BT connection reattempt
CONFIG_BT_NIMBLE_ENABLE_CONN_REATTEMPT=n

#enable lwip ipv6 autoconfig
CONFIG_LWIP_IPV6_AUTOCONFIG=y

# Use a custom partition table
CONFIG_PARTITION_TABLE_CUSTOM=y
CONFIG_PARTITION_TABLE_FILENAME="partitions.csv"
CONFIG_PARTITION_TABLE_OFFSET=0xC000

# Disable chip shell
CONFIG_ENABLE_CHIP_SHELL=n

# Enable OTA Requestor
CONFIG_ENABLE_OTA_REQUESTOR=n

#enable lwIP route hooks
CONFIG_LWIP_HOOK_IP6_ROUTE_DEFAULT=y
CONFIG_LWIP_HOOK_ND6_GET_GW_DEFAULT=y

# disable softap by default
CONFIG_ESP_WIFI_SOFTAP_SUPPORT=n
CONFIG_ENABLE_WIFI_STATION=y
CONFIG_ENABLE_WIFI_AP=n

# Disable DS Peripheral
CONFIG_ESP_SECURE_CERT_DS_PERIPHERAL=n

# Use compact attribute storage mode
CONFIG_ESP_MATTER_NVS_USE_COMPACT_ATTR_STORAGE=y

# Enable HKDF in mbedtls
CONFIG_MBEDTLS_HKDF_C=y

# Increase LwIP IPv6 address number to 6 (MAX_FABRIC + 1)
# unique local addresses for fabrics(MAX_FABRIC), a link local address(1)
CONFIG_LWIP_IPV6_NUM_ADDRESSES=6
