# Enable BLE
CONFIG_BT_ENABLED=y
CONFIG_BT_BLUEDROID_ENABLED=y
CONFIG_BT_BLE_ENABLED=y
CONFIG_BT_BLE_42_FEATURES_SUPPORTED=y
# CONFIG_BT_BLE_50_FEATURES_SUPPORTED is not set

# Enable SMP for security
CONFIG_BT_BLE_SMP_ENABLE=y

# Select crypto library for EAD (Encrypted Advertising Data)
# Options: CONFIG_BT_SMP_CRYPTO_STACK_TINYCRYPT or CONFIG_BT_SMP_CRYPTO_STACK_MBEDTLS
CONFIG_BT_SMP_CRYPTO_STACK_TINYCRYPT=y
